Passive network termination, optical CATV, Outlet SC/PC

Passive network termination, optical CATV, outlet SC/PC,

FTTx customer terminal, passive module for maintaining router freedom for XON30. The module is available in different versions, each for 1- and 2-fiber topologies.

Optimal solution for housing industry, city network operators or energy and utility companies. By inserting the XON1300.P into the XON30 wall bracket, the end customer can commission the connection. Excellent quality and workmanship guarantee longevity and reliability in order to be prepared for future bandwidth requirements.

Supplied without empty housing.

Number of 100 Mbps SC ports (SM): 1

Mounting type: Empty chassis

Ethernet: No

Make: BKtel

Item no.: XON1300.P