FTTH IP65 connection box 8 ports

FTTH IP65 connection box 8 ports,

unassembled 8-ports connection box made of plastic suitable for SC-Simplex/ LC-Duplex/ E2000® couplings, which has an overlength fibre holder. In addition to a swivelling splice cassette, the connection box contains a holder for splitters and a cable sheath.

This box is used in optical telecommunication networks, LAN, CATV networks, FTTH networks as well as PON and G-PON.

Supplied with 8x shrink splice protection and material for wall mounting.

Field of application: Exterior

Mounting type: Wall mounting

Possibility of mast mounting: Yes

Material: plastic

Colour: White

Number of cable entries: 11 (8x max. 3mm / 1x max. 9mm; 2x PG13,5)

Maximum number of fibres: 8

Splice protection type: Shrink / Crimp

Coupling type: SC Simplex/LC Duplex/E2000®

Max. Equipment (adapter): 8

IP Protection class IP65

Protection against foreign bodies and contact: Protection against dust ingress

Water protection: Protection against water jets

Dimensions: hxbxt 213mm x 163mm x 47mm

Temperature range: -25°C - 70°C

Access protection: Special screw

Make: EFB-Elektronik GmbH

Part No.: FTTH-BOX-OUT-2