Wall mount for XON1300 & APL with integrated fiber management

Wall mount for XON1300 & APL with integrated fiber management,

FTTx customer terminal, wall mount for XON1300.P or XON1300.S with overlength fiber holder, whose modularity saves investment and service costs. Optimal solution for housing industry, city network operators or energy and utility companies.

By pre-assembling the bracket as a passive network termination, the active technology can be installed at any time. The XON1300 can be inserted into the rack so that the end customer can commission the connection. An adaptation of the services only requires an exchange of the active module.

Excellent quality and workmanship guarantee longevity and reliability in order to be prepared for future bandwidth requirements. A timeless housing design in the smallest form factor, which was awarded the RedDot Award 2014 for an effective housing concept, fits into every living area.

Area of application: Indoors

Mounting type: Wall mounting

Possibility of mast mounting: No

Material: plastic

Colour: White

Cable entries: 4

Maximum number of fibres: 2

Splice protection type: Crimp / Thermo

Max. Equipment (adapter): 2

IP Protection class IP20

Protection against foreign bodies and accidental contact: Protection against medium-sized foreign bodies

Water protection: No protection

Dimensions: hxbxt 48mm x 150mm x 150mm

Access protection: Without

Make: BKtel

Item no.: XON30