FTTH IP65 connection box 4 ports

FTTH IP65 connection box 4 ports,

unassembled 4-port connection box made of plastic suitable for SC-Simplex/ LC-Duplex/ E2000® couplings, which has an overlength fibre holder. In addition to a swivelling splice cassette, the connection box contains a cable sheathing.

The FTTH IP65 connection box is used in optical telecommunication networks, LAN, CATV networks, FTTH networks as well as PON and G-PON.

Supplied with 4x shrink splice protection and material for wall mounting.

Field of application: Exterior

Mounting type: Wall mounting

Possibility of mast mounting: No

Material: plastic

Colour: White

Number of cable entries: 5 (1x max. 10mm / 4x max. 4mm)

Maximum number of fibres: 4

Splice protection type: Shrink / Crimp

Coupling type: SC Simplex/LC Duplex/E2000®

Max. Equipment (adapter): 4

IP Protection class IP65

Protection against foreign bodies and contact: Protection against dust ingress

Water protection: Protection against water jets

Dimensions: hxbxt 172mm x 136mm x 40mm

Temperature range: -25°C - 70°C

Access protection: Special screw

Make: EFB-Elektronik GmbH

Item no.: FTTH-BOX-OUT-3